Create configuration: C:\Program Files (x86)\PhonerLite\sipper.ini

13:19:28,326: Start of application PhonerLite

13:19:28,326: Loading profiles from configuration file: C:\Program Files (x86)\PhonerLite\sipper.ini

13:19:28,356: Loading profile "sipgate.de" from configuration file: C:\Program Files (x86)\PhonerLite\sipper.ini

13:19:28,356: loading USBphone

13:19:28,476: OpenDevice (sipper.dll)

13:19:28,476: LoadCAPI(sipper.dll)

13:19:28,686: Installed

13:19:28,686: Installed:

13:19:28,686: Get Manufacturer: 53 49 50 50 45 52

13:19:28,686: Get Version: 02 00 00 00 00 00 00 00 01 00 00 00 59 00 00 00

13:19:28,686: SIPPER: 2.0 (1.89)

13:19:28,686: Register: 240 bytes blocksize

13:19:28,686: Register: 00 0C 00 00 02 00 00 00 07 00 00 00 F0 00 00 00

13:19:28,746: Register returns: 01 00 00 00

13:19:28,746: Get Profile: 01 00 08 00 19 00 00 00 03 00 00 00 03 00 00 00 01 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

13:19:28,828: CAPI thread created: 0x0364

13:19:28,854: Listen Request: 1A 00 01 00 05 80 02 00 01 00 00 00 FF 17 00 00 12 00 01 00 00 00 00 00 00 00

13:19:28,854: Listen Request

13:19:28,855: Facility Request: 12 00 01 00 80 80 04 00 01 00 00 00 03 00 03 00 00 00

13:19:28,855: Facility Request (Get Supplementary Services)

-------------------------------------------

13:19:28,833: R: DNS lookup for 'stun.sipgate.net'

start resolving...

-------------------------------------------

13:19:28,944: R: DNS lookup for 'stun.sipgate.net'

217.10.79.2

-------------------------------------------

13:19:28,945: R: DNS lookup for 'sipgate.de'

start resolving SRV (UDP)...

-------------------------------------------

13:19:29,090: R: DNS lookup for 'sipgate.de'

217.10.79.9:5060

-------------------------------------------

13:19:29,091: T: 217.10.79.2:10000

STUN requesting...

-------------------------------------------

13:19:29,180: T: 217.10.79.2:10000

STUN

public ip: 213.162.66.128:37330

-------------------------------------------

13:19:29,180: R: open UDP port (SIP): 5060

-------------------------------------------

13:19:30,026: R: open TCP port (TLS listen): 5061

-------------------------------------------

13:19:30,028: R: open TCP port (TCP listen): 5060

13:19:30,047: Listen Confirm: 0E 00 01 00 05 81 02 00 01 00 00 00 00 00

13:19:30,047: Listen Confirm

-------------------------------------------

13:19:30,034: R: open UDP port (mDNS): 5353

13:19:30,058: Facility Confirm: 1A 00 01 00 80 81 04 00 01 00 00 00 00 00 03 00 09 00 00 06 00 00 3D 01 00 00

13:19:30,058: Facility Confirm (Supplementary Services): Get Supported Services -> success

13:19:30,059: Facility Request: 16 00 01 00 80 80 05 00 01 00 00 00 03 00 07 01 00 04 3D 01 00 00

13:19:30,059: Facility Request (Listen To Supplementary Services)

-------------------------------------------

13:19:30,035: T: 217.10.79.9:5060 (UDP)

REGISTER sip:sipgate.de SIP/2.0

Via: SIP/2.0/UDP 213.162.66.128:37330;branch=z9hG4bK000d4bb6386edf11a7f804f12f145d7f;rport

From: "PhonerLite" <sip:bschlager@sipgate.de>;tag=2565449388

To: "PhonerLite" <sip:bschlager@sipgate.de>

Call-ID: 00E019B5-386E-DF11-A7F7-04F12F145D7F@213.162.66.128

CSeq: 1 REGISTER

Contact: <sip:bschlager@213.162.66.128:37330>;+sip.instance="<urn:uuid:8076B2B5-386E-DF11-A7F8-04F12F145D7F>"

Allow: INVITE, OPTIONS, ACK, BYE, CANCEL, INFO, NOTIFY, MESSAGE, UPDATE

Max-Forwards: 70

User-Agent: SIPPER for PhonerLite

Expires: 900

Content-Length: 0

13:19:30,060: Facility Confirm: 16 00 01 00 80 81 05 00 01 00 00 00 00 00 03 00 05 01 00 02 00 00

13:19:30,061: Facility Confirm (Supplementary Services): Listen -> success

-------------------------------------------

13:19:30,230: R: 217.10.79.9:5060 (UDP)

SIP/2.0 403 Forbidden (No valid Username)

Via: SIP/2.0/UDP 213.162.66.128:37330;branch=z9hG4bK000d4bb6386edf11a7f804f12f145d7f;rport=37522

From: "PhonerLite" <sip:bschlager@sipgate.de>;tag=2565449388

To: "PhonerLite" <sip:bschlager@sipgate.de>;tag=62e0c164533e7d42ac8a2aa4292853db.12ca

Call-ID: 00E019B5-386E-DF11-A7F7-04F12F145D7F@213.162.66.128

CSeq: 1 REGISTER

Content-Length: 0

-------------------------------------------

13:19:30,230: T: 10.106.137.164

STUN disabled because of possible symmetric NAT

-------------------------------------------

13:19:30,231: T: 217.10.79.9:5060 (UDP)

REGISTER sip:sipgate.de SIP/2.0

Via: SIP/2.0/UDP 10.106.137.164:5060;branch=z9hG4bK000d4bb6386edf11a7f904f12f145d7f;rport

From: "PhonerLite" <sip:bschlager@sipgate.de>;tag=2565449388

To: "PhonerLite" <sip:bschlager@sipgate.de>

Call-ID: 00E019B5-386E-DF11-A7F7-04F12F145D7F@10.106.137.164

CSeq: 2 REGISTER

Contact: <sip:bschlager@10.106.137.164:5060>;+sip.instance="<urn:uuid:8076B2B5-386E-DF11-A7F8-04F12F145D7F>"

Allow: INVITE, OPTIONS, ACK, BYE, CANCEL, INFO, NOTIFY, MESSAGE, UPDATE

Max-Forwards: 70

User-Agent: SIPPER for PhonerLite

Expires: 910

Content-Length: 0

-------------------------------------------

13:19:30,350: R: 217.10.79.9:5060 (UDP)

SIP/2.0 403 Forbidden (No valid Username)

Via: SIP/2.0/UDP 10.106.137.164:5060;branch=z9hG4bK000d4bb6386edf11a7f904f12f145d7f;rport=37522;received=213.162.66.128

From: "PhonerLite" <sip:bschlager@sipgate.de>;tag=2565449388

To: "PhonerLite" <sip:bschlager@sipgate.de>;tag=62e0c164533e7d42ac8a2aa4292853db.e0be

Call-ID: 00E019B5-386E-DF11-A7F7-04F12F145D7F@10.106.137.164

CSeq: 2 REGISTER

Content-Length: 0

-------------------------------------------

13:19:30,350: T: 217.10.79.9:5060 (UDP)

REGISTER sip:sipgate.de SIP/2.0

Via: SIP/2.0/UDP 10.106.137.164:5060;branch=z9hG4bK000d4bb6386edf11a7fa04f12f145d7f;rport

From: "PhonerLite" <sip:bschlager@sipgate.de>;tag=2565449388

To: "PhonerLite" <sip:bschlager@sipgate.de>

Call-ID: 00E019B5-386E-DF11-A7F7-04F12F145D7F@10.106.137.164

CSeq: 3 REGISTER

Contact: <sip:bschlager@10.106.137.164:5060>;+sip.instance="<urn:uuid:8076B2B5-386E-DF11-A7F8-04F12F145D7F>"

Allow: INVITE, OPTIONS, ACK, BYE, CANCEL, INFO, NOTIFY, MESSAGE, UPDATE

Max-Forwards: 70

User-Agent: SIPPER for PhonerLite

Expires: 900

Content-Length: 0

-------------------------------------------

13:19:30,460: R: 217.10.79.9:5060 (UDP)

SIP/2.0 403 Forbidden (No valid Username)

Via: SIP/2.0/UDP 10.106.137.164:5060;branch=z9hG4bK000d4bb6386edf11a7fa04f12f145d7f;rport=37522;received=213.162.66.128

From: "PhonerLite" <sip:bschlager@sipgate.de>;tag=2565449388

To: "PhonerLite" <sip:bschlager@sipgate.de>;tag=62e0c164533e7d42ac8a2aa4292853db.7eff

Call-ID: 00E019B5-386E-DF11-A7F7-04F12F145D7F@10.106.137.164

CSeq: 3 REGISTER

Content-Length: 0

13:19:51,090: Listen Request: 1A 00 01 00 05 80 06 00 01 00 00 00 FF 17 00 00 12 00 01 00 00 00 00 00 00 00

13:19:51,091: Listen Request

13:19:51,091: Listen Confirm: 0E 00 01 00 05 81 06 00 01 00 00 00 00 00

13:19:51,091: Listen Confirm

-------------------------------------------

13:19:51,107: R: close UDP port (mDNS): 5353

-------------------------------------------

13:19:51,108: R: open UDP port (mDNS): 5353

-------------------------------------------

13:19:51,108: T: 217.10.79.9:5060 (UDP)

REGISTER sip:sipgate.de SIP/2.0

Via: SIP/2.0/UDP 10.106.137.164:5060;branch=z9hG4bK8065cfc2386edf11a7fa04f12f145d7f;rport

From: "PhonerLite" <sip:bschlager@sipgate.de>;tag=2565449388

To: "PhonerLite" <sip:bschlager@sipgate.de>

Call-ID: 00E019B5-386E-DF11-A7F7-04F12F145D7F@10.106.137.164